**Hydraulic Horsepower**

Where ;

HHP = hydraulic horsepower  
P = circulating pressure (psi)  
Q = circulating rate (gpm)

Case : circulating pressure = 2950 psi  
 circulating rate = 520 gpm

894.98